**Lab 3**

Cascode Amplifier

Part 1: Sizing Chart

Required Spec:

|  |  |
| --- | --- |
| 𝑨 𝒗 = 𝒈𝒎𝒓𝒐 | 50 |
| 𝒈𝒎/𝑰𝑫 | 10 𝑆/𝐴 |
| Supply (𝑽𝑫𝑫) | 1.8 𝑉 |
| Quiescent (DC) output voltage | 𝑉𝐷𝐷/2 = 0.9 𝑉 |
| Bias Current | 20 uA |

Analytic Calculations:




Figure gm/gds vs L

A screenshot of a computer

AI-generated content may be incorrect.

Figure Remaining Parameters @ L = 350nm

**6) W using SA:**

**7)**


****

Figure gm/gds vs VDS Graph

Part 2: Cascode for Gain




Figure CS Amplifier and Cascode Amplifier

Finding VB:

Vds of should be




Figure VDS of M1 vs VB

Ideal value of VB = **1.142V**

DC Operating Point:




Figure DC Voltages Annotated on Schematic

The following table holds the required DC Operating Point parameters for each transistor where: M0 is the CS Amplifier, M1 is Cascode Bottom Transistor, M2 Cascode Top Transistor.

|  |  |  |  |
| --- | --- | --- | --- |
|  | M0 | M1 | M2 |
| ID | 10.0 uA | 10.0 uA | 10.01 uA |
| VGS | 793.4 mV | 798.8 mV | 881.6 mV |
| VDS | 793.4 mV | 258.4 mV | 540.3 mV |
| VTH | 710.1 mV | 710.8 mV | 795.4 mV |
| VDSAT | 135 mV | 138.1 mV | 138.6 mV |
| gm | 124.8 uS | 122.3 uS | 124.2 uS |
| gds | 886.7 nS | 2.61 uS | 1.09 uS |
| gmb | 44.68 uS | 43.81 uS | 38.68 uS |
| Cdb | 544.6 aF | 565.3 aF | 477.9 aF |
| Cgd | 776.7 aF | 847.1 aF | 823.9 aF |
| Cgs | 4.33 fF | 4.42 fF | 4.4 fF |
| Csb | 815.8 aF | 834.1 aF | 714.8 aF |
| Region | 2 | 2 | 2 |

* Check that all transistors operate in saturation.

They all operate in saturation.

* Do all transistors have the same vth? Why?

M0 and M1 have the same VTH as they have the same VSB, but M2 has a higher VTH due to the higher voltage seen at its source.

* What is the relation (≪, <, =, >, ≫) between gm and gds?

gm >> (Much Greater Than) gds

* What is the relation (≪, <, =, >, ≫) between gm and gmb?

gm > (Greater Than) gmb

* What is the relation (≪, <, =, >, ≫) between cgs and cgd?

Cgs >> (Much Greater Than) Cgd

* What is the relation (≪, <, =, >, ≫) between csb and cdb?

Csb > (Greater Than) cdb

AC Analysis:




Figure AC Output Setup


**Outputs:** 

Figure Bode Plots of both CS and Cascode Amplifiers




Figure Gain and UGF Highlighted on Bode Plot

|  |  |  |
| --- | --- | --- |
|  | CS | Cascode |
| Gain (dB) | 42.97 | 77.02 |
| Gain | 140.8 | 7.09 K |
| BW | 140.6 KHz | 2.69 KHz |
| GBW | 19.84 MHz | 19.14 MHz |
| UGF | 19.7956 MHz | 19.1547 MHz |

All Results:

Hand Analysis:

CS Amplifier:

Cascode Amplifier:

Comparison of Results:

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
|  | **CS** | | **Cascode** | |
|  | Simulation | Analytic | Simulation | Analytic |
| **Gain (dB)** | 42.97 | 42.97 | 77.02 | 76.9 |
| **Gain** | 140.8 | 140.75 | 7.09 K | 7 K |
| **BW** | 140.6 KHz | 141.122 KHz | 2.69 KHz | 2.78 KHz |
| **GBW** | 19.84 MHz | 19.863 MHz | 19.14 MHz | 19.46 MHz |
| **UGF** | 19.7956 MHz | 19.863 MHz | 19.1547 MHz | 19.46 MHz |

Comments:

* Simulation and Analytic Results are nearly identical!
* Cascode amplifier has a much greater gain than the CS Amplifier. Due to the higher output resistance
* The Bandwidth of the Cascode Amplifier is much lesser than the CS Amplifier also due to the higher output resistance.
* This results in both amplifiers having nearly identical Gain-Bandwidth-Product as well as Unity Gain Frequency.